|  |  |  |  |
| --- | --- | --- | --- |
| Software Description for Testing | | | |
| Project Name | S800W | Operator | 美标基线 |
| Version Purpose | 可生产测试 | SIM Number | □Single      ■Dual |
| WIND Internal Version No. | WID\_S800W\_K10V1.0B02\_L20150316 | Hardware Version No. | S01 |
| Customer Internal Version No. | N/A | External Version No. | WID\_S800W\_K10V1.0 |
| Branch Info | master | Issue Date | 15/03/16 |
| Baseband Version | MOLY.WR8.W1315.MD.WG.MP.V34.P8 | SIM Lock(Y/N) | N |
| MTK SW Branch Name | ALPS.KK1.MP1.V2.10 | Erase Method | ■Full     □Half |
| Download Method | ■USB      □SD Card | Calibration Method | □UART    ■USB |
| Testing Type  （Entrance/Production/Requirement） | Production | SW Requirement Document | NA |
| Product Outline | Band Info | GSM:850/900/1800/1900 MHz  WCDMA:850/1900 MHz | |
| LCD+TP | qhd | 一供：雅视（OTM9605A）+雅视 (MSG2638M) |
| 二供： 雅视（OTM9605A）+特美克 ( MSG2638M) |
| CPU Info | MT6582 A/W | |
| Main Camera | 一供：OV5648+金康  二供：Hi545+四季春 | |
| Sub Camera | 一供：OV5670+四季春 | |
| 二供：5E2 +凯尔 | |
| G-sensor | LIS3DH,KXCJK-1013 | |
| FLASH Type | Hynix: H9TP65A8JDACPR-KGM (8G)  Toshiba:TYD0GH221640RA(8G) | |
| Android Version | 4.4.2 | |
|  |  | |
| Modifications | 1、后摄：金康和四季春可以做兼容 2、Toshiba H9TP65A8JDACPR-KGM 和Hynix H9TP65A8JDACPR-KGM（老制程的）兼容 | | |
| Special Notes |  | | |
| Version affection |  | | |
| Test Suggestion |  | | |
| RD Self-Test Result | Pass | | |
| Remarks |  | | |
| Claimer | Signature xulinchao  Date 15/03/16 | | |
| SW Department Review | Signature             Date | | |
| Test Department Review | Signature             Date | | |
|  |  | | |