|  |
| --- |
| **[FAQ12046]【sdcard-low storage】Low Storage条件下的相关提示** |

**Platform:**[MT6572](https://onlinesso.mediatek.com/_layouts/15/mol/tag/ext/tagrelateddataview.aspx?tagid=133&tagname=MT6572&type=Platform)[MT6582](https://onlinesso.mediatek.com/_layouts/15/mol/tag/ext/tagrelateddataview.aspx?tagid=144&tagname=MT6582&type=Platform)[MT6589](https://onlinesso.mediatek.com/_layouts/15/mol/tag/ext/tagrelateddataview.aspx?tagid=113&tagname=MT6589&type=Platform)

**Branch:**[JB2](https://onlinesso.mediatek.com/_layouts/15/mol/tag/ext/tagrelateddataview.aspx?tagid=135&tagname=JB2&type=Branch)[JB3](https://onlinesso.mediatek.com/_layouts/15/mol/tag/ext/tagrelateddataview.aspx?tagid=146&tagname=JB3&type=Branch)[JB5](https://onlinesso.mediatek.com/_layouts/15/mol/tag/ext/tagrelateddataview.aspx?tagid=163&tagname=JB5&type=Branch)

|  |
| --- |
| **FAQ Content**  [DESCRIPTION]  Low Storage条件下的相关提示        [SOLUTION]  1)     低于Min（50M，10%\*data区大小）  mMemLowThreshold@alps\frameworks\base\services\java\com\android\server\DeviceStorageMonitorService.java），framework会送Intent.ACTION\_DEVICE\_STORAGE\_LOW intent出去，此时status bar上会有notification  2)     低于10M（[EXCEPTION\_LOW\_THRESHOLD\_BYTES@alps\frameworks\base\services\java\com\android\server\DeviceStorageMonitorService.java](mailto:EXCEPTION_LOW_THRESHOLD_BYTES@alps\frameworks\base\services\java\com\android\server\DeviceStorageMonitorService.java)）, low storage导致的一些APP run time异常，会show dialog提示  C:\Users\xulinchao\Desktop\321.png    3)     低于5M  （FULL\_THRESHOLD\_BYTE S@alps\frameworks\base\services\java\com\android\server\DeviceStorageMonitorService.java），framework会送Intent.ACTION\_DEVICE\_STORAGE\_FULL出去  C:\Users\xulinchao\Desktop\064未命名.bmp  4)     低于4M  CRITICAL\_LOW\_THRESHOLD\_BYTES@alps\frameworks\base\services\java\com\android\server\DeviceStorageMonitorService.java），每隔30s（DEFAULT\_CHECK\_INTERVAL@alps\frameworks\base\services\java\com\android\server\DeviceStorageMonitorService.java）会show “存储空间满”的dialog  C:\Users\xulinchao\Desktop\613.png |